jPicoFishinder_GPS1.0 copy  from jPicoFishinder1.1.1 
//Should set the A to Trigger, B to Signal in the processing box. 
1. dLogData = adc_to_mv(bufPinned[0].Target[i], (short)_channelSettings[(int)Imports.Channel.ChannelB].range); //voltage 
2. Level: 3dB(B=A*1.41)
   

******************************************
jPicoFishinder1.1.1 copy  from 1.1

sPingData--->m_sPingData
in order to use MethodInvoker for debug the multi-thread draw error

jPicoFishinder1.1 copy  from 1.0
1. new UI for display data


jPicoFishinder1.0

1. Use to Log fishfinder data
2. Use multiThread
3. Timer counter and button click to lunch loggingThread
4. Channel A Trigger, Channel B signal

******************************************
Program creation was based on Applied Information System Engineering Laboratory, Ocean Environment Studies Division, Academic Research Institute, Tokyo University of Marine Science and Technology.